Region of Interest

Region of interest was selected based upon the points that were necessary to track the events.

For the circulating event: As shown in the figure below, region A is selected to capture the event when a vehicle passes that point. The difference between the frames gives time event

Approaching event: Region B is selected